{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sanag设备指令测试用例"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sanag设备指令测试用例","index":0,"n_rows":134,"n_cols":12,"rows_kept":134,"cut":false,"hidden":false,"merged":[[0,0,0,11],[2,1,59,1],[60,1,96,1],[97,1,133,1],[3,2,5,2],[6,2,9,2],[10,2,33,2],[34,2,40,2],[41,2,45,2],[46,2,49,2],[50,2,58,2],[61,2,63,2],[64,2,67,2],[68,2,79,2],[80,2,86,2],[87,2,91,2],[92,2,95,2],[98,2,100,2],[101,2,104,2],[105,2,116,2],[117,2,123,2],[124,2,128,2],[129,2,132,2]]}
["sanag Ble蓝牙指令测试用例(根据设备实际功能进行验证)"]
["用例编号","所属模块","二级模块","测试项","类型","优先级","前置条件","操作步骤","预期结果","ios测试结果","安卓测试结果","备注"]
["Sanag_TWS_001","双耳模式","BLE蓝牙连接","验证APP与双耳模式设备进行连接",null,null,null,"使用工具nRF Connect，连接设备BLE蓝牙","连接成功，展示连接UUID=FAA0"]
["Sanag_TWS_002",null,"电量","双耳连接时左耳电量查询",null,null,"成功连接指令工具","使用工具输入 获取左耳电量指令：AA320100DD","响应左耳电量信息，查看倒数第二位，是显示的电量"]
["Sanag_TWS_003",null,null,"双耳连接时右耳电量查询",null,null,"成功连接指令工具","使用工具输入 获取右边耳电量指令：AA330100DE","响应左耳电量信息，查看倒数第二位，是显示的电量"]
["Sanag_TWS_004",null,null,"电量上报",null,null,"成功连接指令工具","查看设备是否成功主动上报左右耳的电量","设备间隔10-30s，设备发送左右耳的电量"]
["Sanag_TWS_005",null,"入耳检测","设置入耳开关设备（开）",null,null,"成功连接指令工具","使用工具输入 打开入耳开关：AA180100C3","返回响应：A5-18-01-00-BE"]
["Sanag_TWS_006",null,null,"设置入耳开关设备（关）",null,null,"成功连接指令工具","使用工具输入 打开入耳开关：AA180101C4","返回响应：A5-18-01-00-BE"]
["Sanag_TWS_007",null,null,"获取当前入耳开关状态（开）",null,null,"成功连接指令工具","使用工具输入 获取入耳模式状态：AA1901FFC3","返回响应：A5-19-01-00-BF（入耳检测开）"]
["Sanag_TWS_008",null,null,"获取当前入耳开关状态（关）",null,null,"成功连接指令工具","使用工具输入 获取入耳模式状态：AA1901FFC3","返回响应：A5-19-01-01-C0（入耳检测关）"]
["Sanag_TWS_009",null,"按键设置","左耳双击设置为播放/暂停",null,null,"成功连接指令工具","使用工具输入 左耳双击指令：AA350100E0","返回响应：A5-35-01-00-DB"]
["Sanag_TWS_010",null,null,"左耳双击设置为上一曲",null,null,"成功连接指令工具","使用工具输入 左耳双击指令：AA350101E1","返回响应：A5-35-01-01-DC"]
["Sanag_TWS_011",null,null,"左耳双击设置为下一曲",null,null,"成功连接指令工具","使用工具输入 左耳双击指令：AA350102E2","返回响应：A5-35-01-02-DD"]
["Sanag_TWS_012",null,null,"左耳双击设置为音量加",null,null,"成功连接指令工具","使用工具输入 左耳双击指令：AA350103E3","返回响应：A5-35-01-03-DE"]
["Sanag_TWS_013",null,null,"左耳双击设置为音量减",null,null,"成功连接指令工具","使用工具输入 左耳双击指令：AA350104E4","返回响应：A5-35-01-04-DF"]
["Sanag_TWS_014",null,null,"获取当前左耳双击状态",null,null,"成功连接指令工具","使用工具输入 获取左耳双击状态：AA3501FFDF","根据设置不同返回响应A5-35-01-00-DB、A5-35-01-01-DC、A5-35-01-02-DD、A5-35-01-03-DE、A5-35-01-04-DF"]
["Sanag_TWS_015",null,null,"右耳双击设置为播放/暂停",null,null,"成功连接指令工具","使用工具输入 右耳双击指令：AA360100E1","返回响应：A5-36-01-00-DC"]
["Sanag_TWS_016",null,null,"右耳双击设置为上一曲",null,null,"成功连接指令工具","使用工具输入 右耳双击指令：AA360101E2","返回响应：A5-36-01-01-DD"]
["Sanag_TWS_017",null,null,"右耳双击设置为下一曲",null,null,"成功连接指令工具","使用工具输入 右耳双击指令：AA360102E3","返回响应：A5-36-01-02-DE"]
["Sanag_TWS_018",null,null,"右耳双击设置为音量加",null,null,"成功连接指令工具","使用工具输入 右耳双击指令：AA360103E4","返回响应：A5-36-01-03-DF"]
["Sanag_TWS_019",null,null,"右耳双击设置为音量减",null,null,"成功连接指令工具","使用工具输入 右耳双击指令：AA360104E5","返回响应：A5-36-01-04-E0"]
["Sanag_TWS_020",null,null,"获取当前右耳双击状态",null,null,"成功连接指令工具","使用工具输入 获取右耳双击状态：AA3601FFE0","根据设置不同返回响应A5-36-01-00-DC、A5-36-01-01-DD、A5-36-01-02-DE、A5-36-01-03-DF、A5-36-01-04-E0"]
["Sanag_TWS_021",null,null,"左耳三击设置为播放/暂停",null,null,"成功连接指令工具","使用工具输入 左耳三击指令：AA370100E2","返回响应：A5-37-01-00-DD"]
["Sanag_TWS_022",null,null,"左耳三击设置为上一曲",null,null,"成功连接指令工具","使用工具输入 左耳三击指令：AA370101E3","返回响应：A5-37-01-01-DE"]
["Sanag_TWS_023",null,null,"左耳三击设置为下一曲",null,null,"成功连接指令工具","使用工具输入 左耳三击指令：AA370102E4","返回响应：A5-37-01-02-DF"]
["Sanag_TWS_024",null,null,"左耳三击设置为音量加",null,null,"成功连接指令工具","使用工具输入 左耳三击指令：AA370103E5","返回响应：A5-37-01-03-E0"]
["Sanag_TWS_025",null,null,"左耳三击设置为音量减",null,null,"成功连接指令工具","使用工具输入 左耳三击指令：AA370104E6","返回响应：A5-37-01-04-E1"]
["Sanag_TWS_026",null,null,"获取当前左耳三击状态",null,null,"成功连接指令工具","使用工具输入 获取左耳三击状态：AA3701FFE1","根据设置不同返回响应A5-37-01-00-DD、A5-37-01-01-DE、A5-37-01-02-DF、A5-37-01-03-E0、A5-37-01-04-E1"]
["Sanag_TWS_027",null,null,"右耳三击设置为播放/暂停",null,null,"成功连接指令工具","使用工具输入 右耳三击指令：AA380100E3","返回响应：A5-38-01-00-DE"]
["Sanag_TWS_028",null,null,"右耳三击设置为上一曲",null,null,"成功连接指令工具","使用工具输入 右耳三击指令：AA380101E4","返回响应：A5-38-01-01-DF"]
["Sanag_TWS_029",null,null,"右耳三击设置为下一曲",null,null,"成功连接指令工具","使用工具输入 右耳三击指令：AA380102E5","返回响应：A5-38-01-02-E0"]
["Sanag_TWS_030",null,null,"右耳三击设置为音量加",null,null,"成功连接指令工具","使用工具输入 右耳三击指令：AA380103E6","返回响应：A5-38-01-03-E1"]
["Sanag_TWS_031",null,null,"右耳三击设置为音量减",null,null,"成功连接指令工具","使用工具输入 右耳三击指令：AA380104E7","返回响应：A5-38-01-04-E2"]
["Sanag_TWS_032",null,null,"获取当前右耳三击状态",null,null,"成功连接指令工具","使用工具输入 获取右耳三击状态：AA3801FFE2","根据设置不同返回响应A5-38-01-00-DE、A5-38-01-01-DF、A5-38-01-02-E0、A5-38-01-03-E1、A5-38-01-04-E2"]
["Sanag_TWS_033",null,"EQ","设置EQ（默认）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390100E4","返回响应：A5-39-01-00-DF"]
["Sanag_TWS_034",null,null,"设置EQ（流行）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390101E5","返回响应：A5-39-01-01-E0"]
["Sanag_TWS_035",null,null,"设置EQ（摇滚）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390102E6","返回响应：A5-39-01-02-E1"]
["Sanag_TWS_036",null,null,"设置EQ（古典）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390103E7","返回响应：A5-39-01-03-E2"]
["Sanag_TWS_037",null,null,"设置EQ（抒情）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390104E8","返回响应：A5-39-01-04-E3"]
["Sanag_TWS_038",null,null,"设置EQ（柔和）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390105E9","返回响应：A5-39-01-05-E4"]
["Sanag_TWS_039",null,null,"获取当前EQ",null,null,"成功连接指令工具","使用工具输入 获取EQ状态：AA76010021","根据不同设置返回响应如：A5-76-01-00-1C"]
["Sanag_TWS_040",null,"游戏模式","设置游戏模式（关）",null,null,"成功连接指令工具","使用工具输入 关闭游戏模式指令：AA290100D4","返回响应：A5-29-01-00-CF"]
["Sanag_TWS_041",null,null,"设置游戏模式（开）",null,null,"成功连接指令工具","使用工具输入 打开游戏模式指令：AA290101D5","返回响应：A5-29-01-00-CF"]
["Sanag_TWS_042",null,null,"获取当前游戏模式（关）",null,null,"成功连接指令工具","使用工具输入 获取游戏模式状态指令：AA410100EC","返回响应：A5-41-01-00-E7"]
["Sanag_TWS_043",null,null,"获取当前游戏模式（开）",null,null,"成功连接指令工具","使用工具输入 获取游戏模式状态指令：AA410100EC","返回响应：A5-41-01-01-E8"]
["Sanag_TWS_044",null,null,"游戏模式上报",null,null,"成功连接指令工具","四击耳机MFB健","上报游戏模式状态，根据实际状态返回A5-41-01-00-E7（关），A5-41-01-01-E8（开）"]
["Sanag_TWS_045",null,"查找耳机","查找双耳耳机",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201000D","返回响应：A5-62-01-00-08"]
["Sanag_TWS_046",null,null,"查找左耳",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201010E","返回响应：A5-62-01-00-08"]
["Sanag_TWS_047",null,null,"查找右耳",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201020F","返回响应：A5-62-01-00-08"]
["Sanag_TWS_048",null,null,"取消查找",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201FF0C","返回响应：A5-62-01-00-08"]
["Sanag_TWS_049",null,"噪音控制","噪音控制（关）",null,null,"成功连接指令工具","使用工具输入 关闭噪音控制指令：AA600200030F","返回响应：A5-60-01-00-06"]
["Sanag_TWS_050",null,null,"噪音控制（降噪模式-轻度）",null,null,"成功连接指令工具","使用工具输入 降躁轻度控制指令：AA600201000D","返回响应：A5-60-01-00-06"]
["Sanag_TWS_051",null,null,"噪音控制（降噪模式-中度）",null,null,"成功连接指令工具","使用工具输入 降躁中度控制指令：AA600201010E","返回响应：A5-60-01-00-06"]
["Sanag_TWS_052",null,null,"噪音控制（降噪模式-重度）",null,null,"成功连接指令工具","使用工具输入 降躁重度控制指令：AA600201020F","返回响应：A5-60-01-00-06"]
["Sanag_TWS_053",null,null,"噪音控制（通透模式-轻度）",null,null,"成功连接指令工具","使用工具输入 通透轻度控制指令：AA600202000E","返回响应：A5-60-01-00-06"]
["Sanag_TWS_054",null,null,"噪音控制（通透模式-中度）",null,null,"成功连接指令工具","使用工具输入 通透轻度控制指令：AA600202010F","返回响应：A5-60-01-00-06"]
["Sanag_TWS_055",null,null,"噪音控制（通透模式-重度）",null,null,"成功连接指令工具","使用工具输入 通透轻度控制指令：AA6002020210","返回响应：A5-60-01-00-06"]
["Sanag_TWS_056",null,null,"获取当前噪音控制状态",null,null,"成功连接指令工具","使用工具输入 获取噪音控制指令：AA6101000C","根据设置不同的噪音模式返回不同结果：\n噪音控制关闭：A5-61-02-00-03-0B\n降噪轻度：A5-61-02-01-00-09\n降噪中度：A5-61-02-01-01-0A\n降噪重度：A5-61-02-01-02-0B\n通透轻度：A5-61-02-02-00-0A\n通透中度：A5-61-02-02-01-0B\n通透中度：A5-61-02-02-02-0C"]
["Sanag_TWS_057",null,null,"设备有噪音控制状态变化需上报状态",null,null,"成功连接指令工具","设备更改降噪模式","需上报状态到APP"]
["Sanag_TWS_058",null,"BLE断开","双耳连接时指令ble断开",null,null,"成功连接指令工具（nRF Connect）","使用工具输入 ble断开指令：AA120100bd","ble 断开连接"]
["Sanag_TWS_059",null,"BLE蓝牙连接","验证APP与左耳模式设备进行连接",null,null,"佩戴左耳，不佩戴右耳","使用工具nRF Connect，连接设备BLE蓝牙","连接成功，展示连接UUID=FAA0"]
["Sanag_TWS_060",null,"电量","双耳连接时左耳电量查询",null,null,"成功连接指令工具","使用工具输入 获取左耳电量指令：AA320100DD","响应左耳电量信息，查看倒数第二位，是显示的电量"]
["Sanag_TWS_061",null,null,"双耳连接时右耳电量查询",null,null,"成功连接指令工具","使用工具输入 获取右边耳电量指令：AA330100DE","响应左耳电量信息，查看倒数第二位，是显示的电量（电量为0）"]
["Sanag_TWS_062",null,null,"电量上报",null,null,"成功连接指令工具","查看设备是否成功主动上报左右耳的电量","设备间隔10-30s，设备发送左右耳的电量"]
["Sanag_TWS_063",null,"入耳检测","设置入耳开关设备（开）",null,null,"成功连接指令工具","使用工具输入 打开入耳开关：AA180100C3","返回响应：A5-18-01-00-BE"]
["Sanag_TWS_064",null,null,"设置入耳开关设备（关）",null,null,"成功连接指令工具","使用工具输入 打开入耳开关：AA180101C4","返回响应：A5-18-01-00-BE"]
["Sanag_TWS_065",null,null,"获取当前入耳开关状态（开）",null,null,"成功连接指令工具","使用工具输入 获取入耳模式状态：AA1901FFC3","返回响应：A5-19-01-00-BF（入耳检测开）"]
["Sanag_TWS_066",null,null,"获取当前入耳开关状态（关）",null,null,"成功连接指令工具","使用工具输入 获取入耳模式状态：AA1901FFC3","返回响应：A5-19-01-01-C0（入耳检测关）"]
["Sanag_TWS_067",null,"按键设置","左耳双击设置为播放/暂停",null,null,"成功连接指令工具","使用工具输入 左耳双击指令：AA350100E0","返回响应：A5-35-01-00-DB"]
["Sanag_TWS_068",null,null,"左耳双击设置为上一曲",null,null,"成功连接指令工具","使用工具输入 左耳双击指令：AA350101E1","返回响应：A5-35-01-01-DC"]
["Sanag_TWS_069",null,null,"左耳双击设置为下一曲",null,null,"成功连接指令工具","使用工具输入 左耳双击指令：AA350102E2","返回响应：A5-35-01-02-DD"]
["Sanag_TWS_070",null,null,"左耳双击设置为音量加",null,null,"成功连接指令工具","使用工具输入 左耳双击指令：AA350103E3","返回响应：A5-35-01-03-DE"]
["Sanag_TWS_071",null,null,"左耳双击设置为音量减",null,null,"成功连接指令工具","使用工具输入 左耳双击指令：AA350104E4","返回响应：A5-35-01-04-DF"]
["Sanag_TWS_072",null,null,"获取当前左耳双击状态",null,null,"成功连接指令工具","使用工具输入 获取左耳双击状态：AA3501FFDF","根据设置不同返回响应A5-35-01-00-DB、A5-35-01-01-DC、A5-35-01-02-DD、A5-35-01-03-DE、A5-35-01-04-DF"]
["Sanag_TWS_073",null,null,"左耳三击设置为播放/暂停",null,null,"成功连接指令工具","使用工具输入 左耳三击指令：AA370100E2","返回响应：A5-37-01-00-DD"]
["Sanag_TWS_074",null,null,"左耳三击设置为上一曲",null,null,"成功连接指令工具","使用工具输入 左耳三击指令：AA370101E3","返回响应：A5-37-01-01-DE"]
["Sanag_TWS_075",null,null,"左耳三击设置为下一曲",null,null,"成功连接指令工具","使用工具输入 左耳三击指令：AA370102E4","返回响应：A5-37-01-02-DF"]
["Sanag_TWS_076",null,null,"左耳三击设置为音量加",null,null,"成功连接指令工具","使用工具输入 左耳三击指令：AA370103E5","返回响应：A5-37-01-03-E0"]
["Sanag_TWS_077",null,null,"左耳三击设置为音量减",null,null,"成功连接指令工具","使用工具输入 左耳三击指令：AA370104E6","返回响应：A5-37-01-04-E1"]
["Sanag_TWS_078",null,null,"获取当前左耳三击状态",null,null,"成功连接指令工具","使用工具输入 获取左耳三击状态：AA3701FFE1","根据设置不同返回响应A5-37-01-00-DD、A5-37-01-01-DE、A5-37-01-02-DF、A5-37-01-03-E0、A5-37-01-04-E1"]
["Sanag_TWS_079",null,"EQ","设置EQ（默认）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390100E4","返回响应：A5-39-01-00-DF"]
["Sanag_TWS_080",null,null,"设置EQ（流行）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390101E5","返回响应：A5-39-01-01-E0"]
["Sanag_TWS_081",null,null,"设置EQ（摇滚）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390102E6","返回响应：A5-39-01-02-E1"]
["Sanag_TWS_082",null,null,"设置EQ（古典）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390103E7","返回响应：A5-39-01-03-E2"]
["Sanag_TWS_083",null,null,"设置EQ（抒情）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390104E8","返回响应：A5-39-01-04-E3"]
["Sanag_TWS_084",null,null,"设置EQ（柔和）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390105E9","返回响应：A5-39-01-05-E4"]
["Sanag_TWS_085",null,null,"获取当前EQ",null,null,"成功连接指令工具","使用工具输入 获取EQ状态：AA76010021","返回响应：A5-76-01-00-1C"]
["Sanag_TWS_086",null,"游戏模式","设置游戏模式（关）",null,null,"成功连接指令工具","使用工具输入 关闭游戏模式指令：AA290100D4","返回响应：A5-29-01-00-CF"]
["Sanag_TWS_087",null,null,"设置游戏模式（开）",null,null,"成功连接指令工具","使用工具输入 打开游戏模式指令：AA290101D5","返回响应：A5-29-01-00-CF"]
["Sanag_TWS_088",null,null,"获取当前游戏模式（关）",null,null,"成功连接指令工具","使用工具输入 获取游戏模式状态指令：AA410100EC","返回响应：A5-41-01-00-E7"]
["Sanag_TWS_089",null,null,"获取当前游戏模式（开）",null,null,"成功连接指令工具","使用工具输入 获取游戏模式状态指令：AA410100EC","返回响应：A5-41-01-01-E8"]
["Sanag_TWS_090",null,null,"游戏模式上报",null,null,"成功连接指令工具","四击耳机MFB健","上报游戏模式状态，根据实际状态返回A5-41-01-00-E7（关），A5-41-01-01-E8（开）"]
["Sanag_TWS_091",null,"查找耳机","查找双耳耳机",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201000D","返回响应：A5-62-01-00-08"]
["Sanag_TWS_092",null,null,"查找左耳",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201010E","返回响应：A5-62-01-00-08"]
["Sanag_TWS_093",null,null,"查找右耳",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201020F","返回响应：A5-62-01-00-08"]
["Sanag_TWS_094",null,null,"取消查找",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201FF0C","返回响应：A5-62-01-00-08"]
["Sanag_TWS_095",null,"BLE断开","左耳连接时指令ble断开",null,null,"成功连接指令工具（nRF Connect）","使用工具输入 ble断开指令：AA120100bd","ble 断开连接"]
["Sanag_TWS_096",null,"BLE蓝牙连接","验证APP与右耳模式设备进行连接",null,null,"佩戴右耳，不佩戴左耳","使用工具nRF Connect，连接设备BLE蓝牙","连接成功，展示连接UUID=FAA0"]
["Sanag_TWS_097",null,"电量","双耳连接时左耳电量查询",null,null,"成功连接指令工具","使用工具输入 获取左耳电量指令：AA320100DD","响应左耳电量信息，查看倒数第二位，是显示的电量"]
["Sanag_TWS_098",null,null,"双耳连接时右耳电量查询",null,null,"成功连接指令工具","使用工具输入 获取右边耳电量指令：AA330100DE","响应左耳电量信息，查看倒数第二位，是显示的电量"]
["Sanag_TWS_099",null,null,"电量上报",null,null,"成功连接指令工具","查看设备是否成功主动上报左右耳的电量","设备间隔10-30s，设备发送左右耳的电量"]
["Sanag_TWS_100",null,"入耳检测","设置入耳开关设备（开）",null,null,"成功连接指令工具","使用工具输入 打开入耳开关：AA180100C3","返回响应：A5-18-01-00-BE"]
["Sanag_TWS_101",null,null,"设置入耳开关设备（关）",null,null,"成功连接指令工具","使用工具输入 打开入耳开关：AA180101C4","返回响应：A5-18-01-00-BE"]
["Sanag_TWS_102",null,null,"获取当前入耳开关状态（开）",null,null,"成功连接指令工具","使用工具输入 获取入耳模式状态：AA1901FFC3","返回响应：A5-19-01-00-BF（入耳检测开）"]
["Sanag_TWS_103",null,null,"获取当前入耳开关状态（关）",null,null,"成功连接指令工具","使用工具输入 获取入耳模式状态：AA1901FFC3","返回响应：A5-19-01-01-C0（入耳检测关）"]
["Sanag_TWS_104",null,null,"右耳双击设置为播放/暂停",null,null,"成功连接指令工具","使用工具输入 右耳双击指令：AA360100E1","返回响应：A5-36-01-00-DC"]
["Sanag_TWS_105",null,null,"右耳双击设置为上一曲",null,null,"成功连接指令工具","使用工具输入 右耳双击指令：AA360101E2","返回响应：A5-36-01-01-DD"]
["Sanag_TWS_106",null,null,"右耳双击设置为下一曲",null,null,"成功连接指令工具","使用工具输入 右耳双击指令：AA360102E3","返回响应：A5-36-01-02-DE"]
["Sanag_TWS_107",null,null,"右耳双击设置为音量加",null,null,"成功连接指令工具","使用工具输入 右耳双击指令：AA360103E4","返回响应：A5-36-01-03-DF"]
["Sanag_TWS_108",null,null,"右耳双击设置为音量减",null,null,"成功连接指令工具","使用工具输入 右耳双击指令：AA360104E5","返回响应：A5-36-01-04-E0"]
["Sanag_TWS_109",null,null,"获取当前右耳双击状态",null,null,"成功连接指令工具","使用工具输入 获取右耳双击状态：AA3601FFE0","根据设置不同返回响应A5-36-01-00-DC、A5-36-01-01-DD、A5-36-01-02-DE、A5-36-01-03-DF、A5-36-01-04-E0"]
["Sanag_TWS_110",null,null,"右耳三击设置为播放/暂停",null,null,"成功连接指令工具","使用工具输入 右耳三击指令：AA380100E3","返回响应：A5-38-01-00-DE"]
["Sanag_TWS_111",null,null,"右耳三击设置为上一曲",null,null,"成功连接指令工具","使用工具输入 右耳三击指令：AA380101E4","返回响应：A5-38-01-01-DF"]
["Sanag_TWS_112",null,null,"右耳三击设置为下一曲",null,null,"成功连接指令工具","使用工具输入 右耳三击指令：AA380102E5","返回响应：A5-38-01-02-E0"]
["Sanag_TWS_113",null,null,"右耳三击设置为音量加",null,null,"成功连接指令工具","使用工具输入 右耳三击指令：AA380103E6","返回响应：A5-38-01-03-E1"]
["Sanag_TWS_114",null,null,"右耳三击设置为音量减",null,null,"成功连接指令工具","使用工具输入 右耳三击指令：AA380104E7","返回响应：A5-38-01-04-E2"]
["Sanag_TWS_115",null,null,"获取当前右耳三击状态",null,null,"成功连接指令工具","使用工具输入 获取右耳三击状态：AA3801FFE2","根据设置不同返回响应A5-38-01-00-DE、A5-38-01-01-DF、A5-38-01-02-E0、A5-38-01-03-E1、A5-38-01-04-E2"]
["Sanag_TWS_116",null,"EQ","设置EQ（默认）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390100E4","返回响应：A5-39-01-00-DF"]
["Sanag_TWS_117",null,null,"设置EQ（流行）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390101E5","返回响应：A5-39-01-01-E0"]
["Sanag_TWS_118",null,null,"设置EQ（摇滚）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390102E6","返回响应：A5-39-01-02-E1"]
["Sanag_TWS_119",null,null,"设置EQ（古典）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390103E7","返回响应：A5-39-01-03-E2"]
["Sanag_TWS_120",null,null,"设置EQ（抒情）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390104E8","返回响应：A5-39-01-04-E3"]
["Sanag_TWS_121",null,null,"设置EQ（柔和）",null,null,"成功连接指令工具","使用工具输入 设置默认EQ：AA390105E9","返回响应：A5-39-01-05-E4"]
["Sanag_TWS_122",null,null,"获取当前EQ",null,null,"成功连接指令工具","使用工具输入 获取EQ状态：AA76010021","返回响应：A5-76-01-00-1C"]
["Sanag_TWS_123",null,"游戏模式","设置游戏模式（关）",null,null,"成功连接指令工具","使用工具输入 关闭游戏模式指令：AA290100D4","返回响应：A5-29-01-00-CF"]
["Sanag_TWS_124",null,null,"设置游戏模式（开）",null,null,"成功连接指令工具","使用工具输入 打开游戏模式指令：AA290101D5","返回响应：A5-29-01-00-CF"]
["Sanag_TWS_125",null,null,"获取当前游戏模式（关）",null,null,"成功连接指令工具","使用工具输入 获取游戏模式状态指令：AA410100EC","返回响应：A5-41-01-00-E7"]
["Sanag_TWS_126",null,null,"获取当前游戏模式（开）",null,null,"成功连接指令工具","使用工具输入 获取游戏模式状态指令：AA410100EC","返回响应：A5-41-01-01-E8"]
["Sanag_TWS_127",null,null,"游戏模式上报",null,null,"成功连接指令工具","四击耳机MFB健","上报游戏模式状态，根据实际状态返回A5-41-01-00-E7（关），A5-41-01-01-E8（开）"]
["Sanag_TWS_128",null,"查找耳机","查找双耳耳机",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201000D","返回响应：A5-62-01-00-08"]
["Sanag_TWS_129",null,null,"查找左耳",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201010E","返回响应：A5-62-01-00-08"]
["Sanag_TWS_130",null,null,"查找右耳",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201020F","返回响应：A5-62-01-00-08"]
["Sanag_TWS_131",null,null,"取消查找",null,null,"成功连接指令工具","使用工具输入 查找双耳指令：AA6201FF0C","返回响应：A5-62-01-00-08"]
["Sanag_TWS_132",null,"BLE断开","右耳连接时指令ble断开",null,null,"成功连接指令工具（nRF Connect）","使用工具输入 ble断开指令：AA120100bd","ble 断开连接"]